

OPTION psf_version = 2.1;

BEGIN DRIVER arduino_io_switch
	OPTION supported_peripherals = (arduino_io_switch);
	OPTION copyfiles = all;
	OPTION VERSION = 1.0;
	OPTION NAME = arduino_io_switch;
END DRIVER
