Quick Start — Python productivity for Zynq (Pynq) v1.0

# Quick Start

To get started with Pynq, follow the quick start instructions below, or read through the documentation for a detailed guide to using Pynq.

## Set up the board

- Set the boot jumper to SD, insert the Micro SD card into the board, and connect the USB cable (Micro-B), and Ethernet cable
- Connect the other end of Ethernet cable to your laptop or router, and the USB cable to your laptop or a powered USB port
- Power on the board, and wait ~30s for the board to boot

## Connect

- Open a browser and go to http://pynq:9090 (board connected to network) or http://192.168.2.99:9090 (board connected to laptop/PC)

The Jupyter password is `xilinx`

## Jupyter Portal

In the Jupyter portal, click on the Welcome to Pynq notebook to get started.

You can find some getting started, and example notebooks in the home area.

## Problems

If you have problems setting up, or connecting to your board, see the full Getting started guide or check the Frequently asked questions

## Support

For support, please go to the support form on the Pynq Webpage www.pynq.io